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PART 1 GENERAL
1.1 SECTION INCLUDES
A. Vinyl shingle siding
B. Vinyl shake siding
C. Vinyl staggered shake siding
D. Vinyl shaped siding
E. Vinyl trim and accessories

1.2 RELATED SECTIONS
A. Section 06100 - Rough Carpentry: Framing and sheathing
B. Section 07900 - Joint Sealers

1.3 REFERENCES
A. ASTM E 84 - Test Method for Surface Burning Characteristics of Building Materials
B. ASTM D 256 - Test Method for Determining the Pendulum Impact Resistance of Notched Specimens of Plastics
C. ASTM D 635 - Test Method for Rate of Burning and/or Extent and Time of Burning of Self-Supported Plastics in a Horizontal Position
D. ASTM D 3679 - Standard Specification for Rigid Poly (Vinyl Chloride) (PVC) Siding
E. VSI - The Vinyl Siding Institute, VSI Product Certification Program
F. VSI - The Vinyl Siding Institute, Vinyl Siding Installation Manual
G. VSI - The Vinyl Siding Institute, Vinyl Siding Cleaning and Maintenance Guide

1.4 SUBMITTALS
A. Submit under provisions of Section 01300
B. Product Data: Manufacturer’s data sheets on each product to be used, including:
1. Preparation instructions and recommendations
2. Storage and handling requirements and recommendation
3. Installation method
C. Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) square, representing actual product, color, and pattern
D. Certificate: Manufacturer’s certification that siding as supplied meets or exceeds the conditions specified herein

1.5 QUALITY ASSURANCE
A. Manufacturer’s Qualifications: Maintain rigorous production quality control standards to ensure that vinyl siding will perform as expected for its intended use. Products meet or exceed the requirements of ICC and VSI and listed
by ICC International Code Council and VSI Vinyl Siding Certification Programs.
B. Regulatory Requirements: Products shall conform with the following:
1. International Code Council - ESR-1728
2. Florida Building Code Commission Report # FL6356
3. Florida Building Code Commission Report # FL14766
4. Texas Department of Insurance Evaluation - EC-51
C. Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship
1. Finish areas designated by Architect
2. Do not proceed with remaining work until workmanship, color, and texture are approved by Architect
3. Refinish mock-up area as required to produce acceptable work
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1.6 DELIVERY, STORAGE, AND HANDLING
A. Pack siding products in cartons and clearly mark each carton with manufacturer’s name, siding style, color, identifying lot number, and VSI Certification Stamp
B. Store products and accessories in clean, dry area, out of direct sunlight
C. Handle material to prevent damage, do not allow cartons to crease

1.2 PROJECT CONDITIONS
A. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer’s absolute limits.
1.8 WARRANTY
A. Upon completion, provide a written transferable, limited lifetime warranty

PART 2 PRODUCTS
2.1 MANUFACTURERS
A. Acceptable Manufacturer: The Foundry® - Westlake Royal Building Products
2801 Post Oak Blvd # 600, Houston, TX 77056; Tel: 800-521-8486; Email: FoundryOrders@westlake.com; Web: www.FoundrySiding.com
B. Requests for substitutions will be considered in accordance with provisions of Section 01600
C. Substitutions: Not permitted

2.2 MATERIALS
A. Vinyl Siding General Requirements: Produced from polyvinyl chloride (PVC) compounds meeting ASTM D 3679 requirements
1. Vinyl Siding Institute Certified
2. Fire Properties:
a. ASTM E 84: Class 1 (A)
1) Flame Spread Index: No more than 25, when tested in accordance with ASTM E 84
2) Smoke Developed Index: No greater than 450, when tested in accordance with ASTM E 84
3) Fuel Contributed: 0
b. Ignition Temperature: When tested in accordance with ASTM D 1929, no self ignition and no flaming; no smoldering at less than 875 degrees F (468 degrees C)
c. Average Time of Burning: Less than 5 seconds, when tested in accordance with ASTM D 635
d. Average Extent of Burning: Less than 5 mm, when tested in accordance with ASTM D 635
3. Typical Siding Properties:
a. Camber: Meet all requirements for camber per ASTM D 3679
b. Heat Shrinkage: Meet all requirements for heat shrinkage per ASTM D 3679
c. Weather Ability: No surface or structural defects such as peeling, cracking, or chipping or blistering when tested per ASTM D 3679
d. Surface Distortion: No distortion at 120 degrees F (40.5 degrees C), per ASTM D 3679
e. Impact Resistance: 60 ft-lbs/in at 20 degrees C when tested in accordance with ASTM D 256
f. Color Formulation: All colors to be formulated with acrylic capstock for fade protection
B. Vinyl Shingles: Foundry Narrow Sawn Cedar Shingle, 7 inch (178 mm)
1. Description: Wood grains are authentic and the appearance of knots, gouges, splits, etc. are considered design features. Twenty different wood grains per panel by 8 panel series = 40 feet no repeat.
2. Width Exposure: 7 inch (178 mm)
3. Length Exposure: 60-3/4 inches (1543 mm)
4. Color: As selected by Architect from manufacturers standards
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C. Vinyl Shingles: Foundry Perfection Shingle, 7 inch (178 mm)
1. Description: Wood grains are authentic and the appearance of knots, gouges, splits, etc. are considered design features. Ten different wood grains per panel by 8 panel series = 40 feet no repeat.
2. Width Exposure: 7 inch (178 mm)
3. Length Exposure: 60-3/4 inches (1543 mm)
D. Vinyl Split Shakes: Foundry Split Shakes, hand split cedar shakes, 7 inch (178 mm)
1. Description: Wood grains are authentic and the appearance of knots, gouges, splits, etc. are considered design features. Ten different wood grains per panel by 8 panel series = 40 feet no repeat.
2. Width Exposure: 7 inch (178 mm)
3. Length Exposure: 60-3/4 inches (1543 mm)
E. Vinyl Staggered Shake: Foundry Staggered Shakes, 7 inch (178 mm) staggered split shakes
1. Description: Wood grains are authentic and the appearance of knots, gouges, splits, etc. are considered design features. Ten different wood grains per panel by 8 panel series = 40 feet no repeat.
2. Width Exposure: 7 inch (178 mm)
3. Length Exposure: 60-3/4 inches (1543 mm)
F. Vinyl Staggered Shake: Foundry Staggered Shakes, 10 inch (254 mm) staggered split shakes
1. Description: Wood grains are authentic and the appearance of knots, gouges, splits, etc. are considered design features. Ten different wood grains per panel by 8 panel series = 40 feet no repeat.
2. Width Exposure: 10 inch (254 mm)
3. Length Exposure: 62-3/4 inches (1594 mm)
G. Vinyl Shapes Round: Foundry round sawn cedar shingle, 6 inch (152 mm)
1. Description: Wood grains are authentic and the appearance of knots, gouges, splits, etc. are considered design features. Ten different wood grains per panel by 8 panel series = 40 feet no repeat.
2. Width Exposure: 6 inch (152 mm)
3. Length Exposure: 60 inches (1524 mm)
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